    ‪©Copyright 2008-2012 Marvell®.‬
    All rights reserved.

    setup_0409.htm created 2012-03-27

    Readme File for SETUP.exe

    Supporting: Marvell Yukon Ethernet Controller

    This package contains the following software components:

    - NDIS5.1 Miniport Driver version 11.45.4.3 for Windows XP/Server 2003 (32 bit)
    - NDIS5.1 Miniport Driver version 11.45.4.3 for Windows XP/Server 2003 (64 bit)
    - NDIS6 Miniport Driver version 11.45.4.3 for Windows Vista/Server 2008 (32 bit)
    - NDIS6 Miniport Driver version 11.45.4.3 for Windows Vista/Server 2008 (64 bit)
    - NDIS6.2 Miniport Driver version 11.45.4.3 for Windows 7 (32 bit)
    - NDIS6.2 Miniport Driver version 11.45.4.3 for Windows 7/Server 2008R2 (64 bit)

# This file contains

1 Overview
2 Required Files
3 Installation

3.1 Driver Installation
3.2 Silent Installation
3.3 Driver Removal
3.4 Silent Removal
3.5 Driver Extraction

4 Further Options
5 Troubleshooting

## 1 Overview

    The driver installation package contains the Marvell NDIS Miniport Driver for the
    Marvell Yukon Ethernet Controller.

    This README file explains how to install the driver installation package on a
    system running one of the following operating systems:

    Windows XP/Server 2003 (x86), Windows XP/Server 2003 (x64), Windows Vista/Server
    2008 (x86), Windows Vista/Server 2008 (x64), Windows 7 (x86), Windows 7/Server
    2008R2 (x64)

    NOTE: Make sure that Windows is installed with the latest Service Packs
          and updates.

## 2 Required Files

    To install the driver, the following file is required:
    - setup.exe

## 3 Installation

    On plug & play Windows versions, the adapter is found, identified, and configured
    automatically. Cancel all operating system attempts to install the driver
    automatically.

    NOTE: To install the driver, you must be logged in as a user
          with administrative rights.

3.1 Driver Installation

    To install the driver, execute the following command:
       setup.exe

3.2 Silent Installation

    To install the driver silently, execute the following command:
       setup.exe /S /LOG=%WINDIR%\YukonInstall.log

3.3 Driver Removal

    To remove the driver, execute the following command:
       setup.exe /REMOVE=ALL

3.4 Silent Removal

    To remove the driver silently, execute the following command:
       setup.exe /S /LOG=%WINDIR%\YukonInstall.log /REMOVE=ALL

3.5 Driver Extraction

    The installer can be used to extract all included Windows drivers for the
    supported Windows operating systems to a directory.

    To extract the drivers to the directory where the setup.exe is located, execute
    the following command:
       setup.exe /E

    To extract the drivers to a specific directory, execute the following command:
       setup.exe /E=<extraction path>

## 4 Further Options

    By default, the installation directory is "%PROGRAMFILES%\Marvell\Miniport
    Driver". It can be changed by setting the variable "INSTALLDIR".

    Example:
       setup.exe /S /LOG=%WINDIR%\YukonInstall.log /INSTALLDIR=C:\MyDir

    The installation status is logged in the file "%WINDIR%\YukonInstall.log". The
    log file path and name can be changed by replacing "%WINDIR%\YukonInstall.log"
    with the preferred file path and name.

## 5 Troubleshooting

    If you should encounter any problems with your driver installation package,
    please re-read the instructions above and the documentation supplied with the
    operating system carefully.

    Additionally, refer to your system event log file (using the Event Viewer), and
    check it for entries from the Marvell NDIS Miniport Driver. If your particular
    problem is not listed or the error persists, please send your system event log
    file to our technical support.

    For further information, please contact our support.

    *** End of Readme File ***