______________________________________________________________________________

ReadMe.txt
______________________________________________________________________________

Copyright (C) 2007 Oxford Semiconductor Ltd.

Device driver for legacy mode UARTs of PCIe952 device family.

____________________________
Installation
____________________________

1. Install Windows CE 4.2 Platform Builder (PB) to a development PC. Note the 
   WINCEROOT i.e. the path where WinCE 4.2 is installed (generally C:\WINCE420)

2. Execute the batch file "CopyDriverToWinCERoot.bat" which will prompt the user
   to enter the WINCEROOT. The batch file will then copy all the files to the 
   WINCEROOT. The following directory structure shall be seen:
   
	C:\WINCE420\OXSEMI
	               |------UARTS
	               |        |
	               |        |-----....
	               |        |-----PCIE952_UART
	               |        |-----INC
	               |        \-----....
	               |
	               \------....

3. Start Platform Builder and create a new platform.

4. Click “File->Manage Catalog Features” to start “Manage Catalog Features” dialog

5. Click “Import…” button to start “Import Catalog Features” dialog and import 
   cec files of “pcie952_uart.cec” in the subdirectory of “\uarts\pcie952_uart\"

6. Add "COM16550" feature to the platform by right-click on its logo and choose
   “Add to Platform”

7. Add "pcie952_uart" feature to the platform by right-click on its logo and
   click on “Add to Platform”

8. Start platform build process by clicking “Build OS->Build and Sysg" or simply
   remake the OS image by "Build OS->Make Run-Time Image" if a image is existing
________________________________________________________________________________

                                 End of ReadMe
________________________________________________________________________________
