CECInfo
(
	Name ( "GpioDriver" )
	CECVersion ( 5.00 )
	GUID ( {BD43BA3D-B66A-4159-9CEE-C313E41DA388} )
)
ComponentType
(
	Name ( "Gpio" )
	GUID ( {B82862F3-6816-4B06-ABD2-EE02C6050733} ) 
	Group ( "\device drivers\Gpio" )
	Vendor ( "oxsemi" )
	MaxResolvedImpsAllowed( 999 )
	Implementations
	(
		Implementation
		(
			Name ( "Gpio" )
			GUID ( {3E57A912-5EBC-4993-8A98-B0F183C61DB9} )
			Version ( "1.0.0.0" )
			Locale ( 0409 )
			Vendor ( "oxsemi" )
			Date ( "29/10/2007" )
			SizeIsCPUDependent( 1 )
			BuildMethods
			(
				BuildMethod
				(
					GUID ( {D0135395-B845-47E8-B97D-C9F821658CBE} )
					Step ( CESYSGEN )
					CPU ( "ARMV4I" )
					CPU ( "x86" )
					Action ( '#SRCCODE( USER_PROJECT, "$(_WINCEROOT)\OXSEMI\GPIOs\Gpio\GpioDriver.pbpxml" )' )
				)
			)
		)
	)
) 
