--- old/drivers/parport/parport_pc.c	2006-05-11 02:56:24.000000000 +0100
+++ new/drivers/parport/parport_pc.c	2006-11-24 12:37:54.000000000 +0100
@@ -2750,6 +2750,7 @@
 	avlab_2p,
 	oxsemi_954,
 	oxsemi_840,
+	oxsemi_pcie_pport,
 	aks_0100,
 	mobility_pp,
 	netmos_9705,
@@ -2825,6 +2826,7 @@
 	 * and 840 locks up if you write 1 to bit 2! */
 	/* oxsemi_954 */		{ 1, { { 0, -1 }, } },
 	/* oxsemi_840 */		{ 1, { { 0, -1 }, } },
+	/* oxsemi_pcie_pport */		{ 1, { { 0, 1 }, } },
 	/* aks_0100 */                  { 1, { { 0, -1 }, } },
 	/* mobility_pp */		{ 1, { { 0, 1 }, } },
 	/* netmos_9705 */               { 1, { { 0, -1 }, } }, /* untested */
@@ -2884,7 +2886,6 @@
 	{ 0x1409, 0x7268, 0x1409, 0x0103, 0, 0, timedia_4008a },
 	{ 0x1409, 0x7268, 0x1409, 0x0104, 0, 0, timedia_4018 },
 	{ 0x1409, 0x7268, 0x1409, 0x9018, 0, 0, timedia_9018a },
-	{ 0x14f2, 0x0121, PCI_ANY_ID, PCI_ANY_ID, 0, 0, mobility_pp },
 	{ PCI_VENDOR_ID_SYBA, PCI_DEVICE_ID_SYBA_2P_EPP,
 	  PCI_ANY_ID, PCI_ANY_ID, 0, 0, syba_2p_epp },
 	{ PCI_VENDOR_ID_SYBA, PCI_DEVICE_ID_SYBA_1P_ECP,
@@ -2900,8 +2901,25 @@
 	  PCI_ANY_ID, PCI_ANY_ID, 0, 0, oxsemi_954 },
 	{ PCI_VENDOR_ID_OXSEMI, PCI_DEVICE_ID_OXSEMI_12PCI840,
 	  PCI_ANY_ID, PCI_ANY_ID, 0, 0, oxsemi_840 },
+	{ PCI_VENDOR_ID_OXSEMI, PCI_DEVICE_ID_OXSEMI_PCIe840,
+	  PCI_ANY_ID, PCI_ANY_ID, 0, 0, oxsemi_pcie_pport },
+	{ PCI_VENDOR_ID_OXSEMI, PCI_DEVICE_ID_OXSEMI_PCIe840_G,
+	  PCI_ANY_ID, PCI_ANY_ID, 0, 0, oxsemi_pcie_pport },
+	{ PCI_VENDOR_ID_OXSEMI, PCI_DEVICE_ID_OXSEMI_PCIe952_0,
+	  PCI_ANY_ID, PCI_ANY_ID, 0, 0, oxsemi_pcie_pport },
+	{ PCI_VENDOR_ID_OXSEMI, PCI_DEVICE_ID_OXSEMI_PCIe952_0_G,
+	  PCI_ANY_ID, PCI_ANY_ID, 0, 0, oxsemi_pcie_pport },
+	{ PCI_VENDOR_ID_OXSEMI, PCI_DEVICE_ID_OXSEMI_PCIe952_1,
+	  PCI_ANY_ID, PCI_ANY_ID, 0, 0, oxsemi_pcie_pport },
+	{ PCI_VENDOR_ID_OXSEMI, PCI_DEVICE_ID_OXSEMI_PCIe952_1_G,
+	  PCI_ANY_ID, PCI_ANY_ID, 0, 0, oxsemi_pcie_pport },
+	{ PCI_VENDOR_ID_OXSEMI, PCI_DEVICE_ID_OXSEMI_PCIe952_1_U,
+	  PCI_ANY_ID, PCI_ANY_ID, 0, 0, oxsemi_pcie_pport },
+	{ PCI_VENDOR_ID_OXSEMI, PCI_DEVICE_ID_OXSEMI_PCIe952_1_GU,
+	  PCI_ANY_ID, PCI_ANY_ID, 0, 0, oxsemi_pcie_pport },
 	{ PCI_VENDOR_ID_AKS, PCI_DEVICE_ID_AKS_ALADDINCARD,
 	  PCI_ANY_ID, PCI_ANY_ID, 0, 0, aks_0100 },
+	{ 0x14f2, 0x0121, PCI_ANY_ID, PCI_ANY_ID, 0, 0, mobility_pp },
 	/* NetMos communication controllers */
 	{ PCI_VENDOR_ID_NETMOS, PCI_DEVICE_ID_NETMOS_9705,
 	  PCI_ANY_ID, PCI_ANY_ID, 0, 0, netmos_9705 },
--- old/include/linux/pci_ids.h	2006-05-11 02:56:24.000000000 +0100
+++ new/include/linux/pci_ids.h	2006-11-24 12:37:54.000000000 +0100
@@ -1807,6 +1807,14 @@
 
 #define PCI_VENDOR_ID_OXSEMI		0x1415
 #define PCI_DEVICE_ID_OXSEMI_12PCI840	0x8403
+#define PCI_DEVICE_ID_OXSEMI_PCIe840		0xC000
+#define PCI_DEVICE_ID_OXSEMI_PCIe840_G		0xC004
+#define PCI_DEVICE_ID_OXSEMI_PCIe952_0		0xC100
+#define PCI_DEVICE_ID_OXSEMI_PCIe952_0_G	0xC104
+#define PCI_DEVICE_ID_OXSEMI_PCIe952_1		0xC110
+#define PCI_DEVICE_ID_OXSEMI_PCIe952_1_G	0xC114
+#define PCI_DEVICE_ID_OXSEMI_PCIe952_1_U	0xC118
+#define PCI_DEVICE_ID_OXSEMI_PCIe952_1_GU	0xC11C
 #define PCI_DEVICE_ID_OXSEMI_16PCI954	0x9501
 #define PCI_DEVICE_ID_OXSEMI_16PCI95N	0x9511
 #define PCI_DEVICE_ID_OXSEMI_16PCI954PP	0x9513
